Bus and Coach Walkaround Check
A bus and coach (PSV) daily walkaround check and defect report: the 29 DVSA checks from the driver's seat, inside and outside, tyre tread, each defect graded dangerous or not with photos, who it was reported to, and repair.
1. Vehicle
Project
______________________________________________________________________________
Client
______________________________________________________________________________
Site *
______________________________________________________________________________
Site address
______________________________________________________________________________
Check date *
______________________________________________________________________________
Time
______________________________________________________________________________
Registration or identification mark *
______________________________________________________________________________
Fleet number
______________________________________________________________________________
Vehicle  (choose one)
☐ Single-deck bus     ☐ Double-deck bus     ☐ Coach     ☐ Minibus
Odometer reading
______________________________________________________________________________
Checked by *
______________________________________________________________________________
Check done by  (choose one)
☐ The driver     ☐ A responsible person (not the driver)
	DVSA: carry out a walkaround check before the journey to make sure the vehicle is safe, and report any defects in writing to the person in charge of sorting out vehicle defects. DVSA's guide to maintaining roadworthiness says at least one walkaround check must be done every day, or once in each 24-hour period, that the vehicle is used.



	If applicable: Where the check is done by a responsible person, DVSA says the driver needs to see evidence that it was done and that the vehicle is free from safety defects.



2. From the driver's seat
1. Front view: mirrors, cameras and glass in place, windscreen not cracked, nothing blocking the view  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
2. Windscreen wipers and washers work, wipers not missing, damaged or worn  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
3. Instruments, gauges and warning lamps work, including ABS, full headlamp and parking brake  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
4. Steering moves properly, power steering works, no excessive play  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
5. Horn works and is easy to reach  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
6. Air builds up, warning system works, no air leaks, service and parking brakes work  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
7. Height marker in the cab shows the vehicle height  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
8. Electronic ticket machine working  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
9. Driver's seat belt undamaged, latches and retracts  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
3. Inside the vehicle
10. Doors and emergency exits work, secure when shut, markings visible and lights working  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
11. Accessibility: wheelchair space, boarding device, priority seats, handrails, colour contrast  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
12. Seats secure and undamaged, seat belts undamaged, latch and retract  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
13. Bell pushes, stopping signs and route and destination signs work  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
14. Heating, ventilation and de-misters work, windows and roof hatches secure  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
15. Emergency exit hammers present and easy to reach  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
16. Fire extinguisher correct type, easy to reach, in good condition, not discharged  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
17. First aid kit present, in good condition and easy to reach (where required)  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
18. Body interior: exits clear, floor and steps sound, rails secure, interior lights work  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
4. Outside the vehicle
19. Tyres and wheels secure, tread at least 1mm, inflated, no deep cuts or cord, wheel nuts in place  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
20. Lights, indicators, side repeaters and reflectors work, clean, right colour  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
21. Number plate not broken, incorrect, dirty, faded or covered  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
22. Body panels, luggage and access doors secure, no jagged edges  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
23. Fuel filler cap fitted, no fuel, oil or waste leaks  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
24. No excessive exhaust smoke  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
25. AdBlue (diesel exhaust fluid) topped up  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
26. Battery secure, in good condition, not leaking (if easily accessible)  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
27. Ancillary equipment secure and working  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
28. High voltage emergency cut-off switch located and working, components secure  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
29. Alternative fuel system: isolation switch located, no leaks, components in good condition  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
Lowest tyre tread depth found (mm)
______________________________________________________________________________
	If applicable: Below the 1mm minimum tread depth in DVSA's walkaround check. Do not use the vehicle until the tyre is replaced.



Have any wheel nut indicators moved?
☐ Yes     ☐ No
Walk Cam: bus and coach walkaround check
Walk Cam video walk-through: available in the SiteSurvey app only.
5. Defect report
Were any defects found? *
☐ Yes     ☐ No
	If applicable: No defects: this record is the nil defect report. DVSA says to record nil defects if you do not find any.



Defects  (copy this block for each one; if applicable)
Item and defect *
______________________________________________________________________________
Assessment *  (choose one)
☐ Dangerous: do not use     ☐ Not dangerous: report for repair
Photos  (photos: attach, or note the file names)
______________________________________________________________________________
Dangerous defects  (if applicable; worked out automatically in the app)
______________________________________________________________________________
	If applicable: DVSA: dangerous defects must be fixed before the vehicle is used or continues its journey.



Reported to  (if applicable)
______________________________________________________________________________
Time reported  (if applicable)
______________________________________________________________________________
Vehicle status *  (choose one)
☐ Roadworthy: safe to use     ☐ Not to be used until repaired
	DVSA's guide to maintaining roadworthiness: drivers' defect reports, with any rectification work, must be kept for at least 15 months.



6. Repair and sign-off
Rectification work done  (if applicable)
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
Repaired by  (if applicable)
______________________________________________________________________________
Repair date  (if applicable)
______________________________________________________________________________
Vehicle confirmed roadworthy after repair?  (if applicable)
☐ Yes     ☐ No
Driver or checker name *
______________________________________________________________________________
Signature
	



Defect report received by (transport or engineering)
______________________________________________________________________________
Signature
	



Bus and Coach Walkaround Check. Printable copy from the SiteSurvey form library. Fill it in on a phone, with photos and signatures: sitesurvey.app/forms/bus-walkaround-check/




