Conveyor Belt Inspection
A belt conveyor inspection: whether it was running or isolated, belt surface, edges, tracking and joints, rollers and drums, spillage, guards, pull cords and emergency stops, result, photos and repair actions.
1. Conveyor
Project
______________________________________________________________________________
Client
______________________________________________________________________________
Site *
______________________________________________________________________________
Site address
______________________________________________________________________________
Inspection date *
______________________________________________________________________________
Time
______________________________________________________________________________
Inspector *
______________________________________________________________________________
Conveyor reference *
______________________________________________________________________________
Type  (choose one)
☐ Flat belt
☐ Troughed belt
☐ Incline or decline belt
☐ Modular plastic belt
☐ Other
State during the inspection *  (choose one)
☐ Running: checked from the walkway only     ☐ Stopped and isolated: locked off
Isolation point and personal lock  (if applicable)
______________________________________________________________________________
	Do not remove a guard or reach in while the conveyor can move. HSE advises, in its quarries guidance, that cleaning and maintenance of conveyors must only be done when the conveyor is properly isolated and the isolator locked with a personal lock and key, and that pull wires are additional protection, not an alternative to fixed guards.



	PUWER regulation 11 requires measures to prevent access to dangerous parts of machinery, with fixed guards where practicable, kept in efficient working order and good repair. Regulation 6 requires inspection at suitable intervals where equipment is exposed to deterioration, and HSE says the result should be recorded and kept at least until the next inspection.



2. Checks
Walkways and access clear  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
Belt surface: no cuts, tears or worn patches  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
Belt edges: no fraying  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
Belt runs centrally (tracking)  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
Belt joint or fasteners  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
Rollers and idlers turn freely, none seized  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
Head and tail drums  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
No spillage or build-up under the belt  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
Fixed guards in place at drives, drums and nip points  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
Pull cord, where fitted, runs head to tail and stops the belt  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
Emergency stop buttons  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
Isolation point clearly marked and lockable  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
	If applicable: A missing or damaged guard. Keep the conveyor out of use until it is refitted or repaired: PUWER regulation 11 requires guards to be maintained in an efficient state and in good repair.



	If applicable: PUWER regulation 16 requires readily accessible emergency stop controls where appropriate. Report a faulty stop or pull cord before the conveyor is used.



Photos (from outside the guards)  (photos: attach, or note the file names)
______________________________________________________________________________
Walk Cam: conveyor belt inspection
Walk Cam video walk-through: available in the SiteSurvey app only.
3. Actions and sign-off
Overall result *  (choose one)
☐ Safe to use     ☐ Safe to use: repairs booked     ☐ Out of use
Are further actions needed?
☐ Yes     ☐ No
Further actions  (copy this block for each one; if applicable)
What needs doing? *
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
Who will do it?
______________________________________________________________________________
Due date
______________________________________________________________________________
Status  (choose one)
☐ Open     ☐ In progress     ☐ Completed
Inspector name *
______________________________________________________________________________
Position or company
______________________________________________________________________________
Inspector signature
	



	Signing records what was found on the day. It does not make unsafe equipment safe or replace a thorough examination, design check or service by a competent person.



Conveyor Belt Inspection. Printable copy from the SiteSurvey form library. Fill it in on a phone, with photos and signatures: sitesurvey.app/forms/conveyor-belt-inspection-checklist/




