Highway and Car Park Safety Inspection
A highway, footway and car park safety inspection: route, hierarchy and inspection type, each defect with its type, size, response category and photos, made safe, and actions.
1. Inspection
Project
______________________________________________________________________________
Client
______________________________________________________________________________
Site *
______________________________________________________________________________
Site address
______________________________________________________________________________
Inspection date *
______________________________________________________________________________
Time
______________________________________________________________________________
Inspector *
______________________________________________________________________________
Route, street or car park *
______________________________________________________________________________
Network hierarchy or category
______________________________________________________________________________
Inspection  (choose one)
☐ Routine (cyclic) safety inspection
☐ Reactive, after a report
☐ Night inspection (lighting)
Method  (choose one)
☐ Walked     ☐ Driven
Your investigatory level: carriageway or car park depth (mm)
Optional. From your own inspection policy. The code of practice leaves these levels to each authority or owner.
______________________________________________________________________________
Footway trip height (mm)
Optional. From your own inspection policy.
______________________________________________________________________________
	For public highways in England and Wales, section 58 of the Highways Act 1980 gives the highway authority a defence to a claim if it took the care reasonably required, and the court considers whether it knew, or could reasonably have known, of the danger. The UK Roads Liaison Group code of practice says inspection records are crucial to defending claims, and that nil returns should be recorded too.



Weather capture
Digital form: use Record current conditions. On paper, record date/time, temperature (°C), wind (mph and direction), conditions and source. Keep observed conditions separate from forecast estimates.
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
2. Defects
Were any defects found?
☐ Yes     ☐ No
Defects  (copy this block for each one; if applicable)
Defect *  (choose one)
☐ Pothole
☐ Trip hazard on footway
☐ Kerb damage
☐ Ironwork or cover
☐ Signs
☐ Road markings
☐ Lighting
☐ Gully or drainage
☐ Vegetation or sight lines
☐ Barrier or bollard
☐ Other
Location (house number, bay, lamp column) *
______________________________________________________________________________
Where it is (GPS)
Optional. Mark the defect so the repair gang finds it.
______________________________________________________________________________
What is wrong?
______________________________________________________________________________
Depth or height (mm)
By a ruler or gauge at the deepest point or the highest edge.
______________________________________________________________________________
Width (mm)
Use a tape, or measure from a photo looking straight down, with a rule or a known bay line in the same plane.
______________________________________________________________________________
Length (mm)
______________________________________________________________________________
Area (m²)  (if applicable; worked out automatically in the app)
______________________________________________________________________________
Against your investigatory level  (if applicable; worked out automatically in the app)
______________________________________________________________________________
Response *  (choose one)
☐ Make safe within 24 hours
☐ Repair within 28 days
☐ Planned works
☐ Monitor at next inspection
Made safe on site (coned or signed)?  (if applicable)
☐ Yes     ☐ No
Photos (with a scale if possible)  (photos: attach, or note the file names)
______________________________________________________________________________
is_over  (worked out automatically in the app)
______________________________________________________________________________
is_unsafe  (worked out automatically in the app)
______________________________________________________________________________
is_area  (worked out automatically in the app)
______________________________________________________________________________
	If applicable: Not made safe on site. Cone or sign it now, or arrange the response within 24 hours, and record who was told.



Defects needing action within 24 hours  (if applicable; worked out automatically in the app)
______________________________________________________________________________
Defects to repair within 28 days  (if applicable; worked out automatically in the app)
______________________________________________________________________________
Planned works  (if applicable; worked out automatically in the app)
______________________________________________________________________________
Monitor at the next inspection  (if applicable; worked out automatically in the app)
______________________________________________________________________________
At or over your investigatory level  (if applicable; worked out automatically in the app)
______________________________________________________________________________
24-hour defects not made safe  (if applicable; worked out automatically in the app)
______________________________________________________________________________
Area to repair (m²)  (if applicable; worked out automatically in the app)
______________________________________________________________________________
	If applicable: A defect needing action within 24 hours was not made safe on site. Arrange it now and record who was told.



	Well-managed Highway Infrastructure, the UK Roads Liaison Group code of practice, is not statutory. Its 2016 edition recommends a risk-based inspection regime, with each authority setting inspection frequencies by the network hierarchy and recording defects with a response based on risk. The response categories here are examples: use your own policy.



Walk Cam: route inspection
Walk Cam video walk-through: available in the SiteSurvey app only.
3. Actions and sign-off
Are further actions needed?
☐ Yes     ☐ No
Further actions  (copy this block for each one; if applicable)
What needs doing? *
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
Priority  (choose one)
☐ Urgent     ☐ High     ☐ Medium     ☐ Low
Who will do it?
______________________________________________________________________________
Due date
______________________________________________________________________________
Status  (choose one)
☐ Open     ☐ In progress     ☐ Completed
Actions open or in progress  (if applicable; worked out automatically in the app)
______________________________________________________________________________
Next inspection due
Set by the inspection frequency the authority or owner has set for this hierarchy category.
______________________________________________________________________________
Days to next due  (if applicable; worked out automatically in the app)
______________________________________________________________________________
	If applicable: The next inspection due date is before the inspection date. Check the date.



Inspector name *
______________________________________________________________________________
Position or company
______________________________________________________________________________
Inspector signature
	



	Signing records what was found on the day. It does not make unsafe equipment safe or replace a thorough examination, design check or service by a competent person.



Highway and Car Park Safety Inspection. Printable copy from the SiteSurvey form library. Fill it in on a phone, with photos and signatures: sitesurvey.app/forms/highway-inspection-checklist/




