Pallet Racking Inspection
A pallet racking inspection: damage by aisle, bay and level with green, amber and red ratings, offload actions, general checks and the date of the last expert inspection.
1. Inspection details
Project
______________________________________________________________________________
Client
______________________________________________________________________________
Site *
______________________________________________________________________________
Site address
______________________________________________________________________________
Date of inspection *
______________________________________________________________________________
Time
______________________________________________________________________________
Warehouse, area or aisles inspected *
______________________________________________________________________________
Inspected by *
______________________________________________________________________________
Person responsible for racking safety (PRRS)
The named person who manages racking safety on site and sets how often it is inspected.
______________________________________________________________________________
Type of inspection *  (choose one)
☐ Regular in-house inspection (weekly or as set by the PRRS)
☐ After an impact or reported damage
☐ Expert inspection by a technically competent person
Date of the last expert inspection
______________________________________________________________________________
Days since the expert inspection  (if applicable; worked out automatically in the app)
______________________________________________________________________________
	If applicable: More than 12 months since the expert inspection. HSE warehousing guidance (HSG76) says a technically competent person should inspect racking at intervals of not more than 12 months, alongside regular in-house inspections like this one.



2. Damage found
	Damage categories (HSE HSG76, table 11, based on SEMA guidance). Green: within the limit, safe for further service; record it and look at it again at later inspections. Amber: hazardous damage needing action as soon as possible; once the load is removed, do not reload it until repaired. Amber damage not repaired within 4 weeks should be treated as red. Red: very serious damage; offload and isolate the area immediately until repaired.



Did you find any damage?
☐ Yes     ☐ No
Damage  (copy this block for each one; if applicable)
Aisle, bay and beam level *
______________________________________________________________________________
Component *  (choose one)
☐ Upright
☐ Beam
☐ Bracing (diagonal or horizontal)
☐ Base plate or floor fixing
☐ Beam connector or safety lock
☐ Decking or pallet support
☐ Column guard
☐ Other
What is the damage? *
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
Category *  (choose one)
☐ Green: record and watch     ☐ Amber: repair soon     ☐ Red: offload now
	If applicable: Amber. Do not put new loads on this rack once it is emptied, and arrange a repair within 4 weeks.



Is it labelled so it is not reloaded until repaired?  (if applicable)
☐ Yes     ☐ No
	If applicable: Red. Offload the affected racking now and keep it out of use until it has been repaired.



Has it been offloaded and isolated?  (if applicable)
☐ Yes     ☐ No
Repair by (who and date)  (if applicable)
______________________________________________________________________________
Photos  (photos: attach, or note the file names)
______________________________________________________________________________
Red items  (if applicable; worked out automatically in the app)
______________________________________________________________________________
Amber items  (if applicable; worked out automatically in the app)
______________________________________________________________________________
Green items  (if applicable; worked out automatically in the app)
______________________________________________________________________________
Walk Cam: racking damage visual inspection
Walk Cam video walk-through: available in the SiteSurvey app only.
3. General checks
Load notices displayed, readable and matching the configuration  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
Floor fixings in place, floor not cracked or uneven  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
Beam safety locks fitted on every beam  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
Column guards and end-of-aisle protectors in place and undamaged  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
Uprights plumb, no visible lean or bowing  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
Loads within the rated capacity, pallets sound and sitting squarely  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
Decking, mesh and pallet supports in place  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
Aisles clear, no items stored in flue spaces or on the floor in front  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
No unauthorised changes to beam levels or configuration  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
Photos  (photos: attach, or note the file names)
______________________________________________________________________________
4. Actions and sign-off
Overall result *  (choose one)
☐ No damage needing action
☐ Repairs needed (amber)
☐ Areas offloaded and isolated (red)
Summary for the PRRS
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
Are further actions needed?
☐ Yes     ☐ No
Further actions  (copy this block for each one; if applicable)
What needs doing? *
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
Who will do it?
______________________________________________________________________________
Due date
______________________________________________________________________________
Status  (choose one)
☐ Open     ☐ In progress     ☐ Completed
Inspector name *
______________________________________________________________________________
Position or company
______________________________________________________________________________
Inspector signature
	



	Signing records what was found on the day. It does not make unsafe equipment safe or replace a thorough examination, design check or service by a competent person.



Pallet Racking Inspection. Printable copy from the SiteSurvey form library. Fill it in on a phone, with photos and signatures: sitesurvey.app/forms/pallet-racking-inspection-checklist/




