Retrofit Assessment Record
A whole-house retrofit assessment data record (PAS 2035 style): dwelling, construction, condition, ventilation, heating and hot water, existing measures, occupancy, defects to fix first and photos.
1. Dwelling
Project
______________________________________________________________________________
Client
______________________________________________________________________________
Site *
______________________________________________________________________________
Site address
______________________________________________________________________________
Assessment date *
______________________________________________________________________________
Time
______________________________________________________________________________
Retrofit assessor *
______________________________________________________________________________
Dwelling type  (choose one)
☐ Detached
☐ Semi-detached
☐ Mid-terrace
☐ End-terrace
☐ Flat
☐ Maisonette
☐ Bungalow
Age  (choose one)
☐ Before 1900
☐ 1900 to 1929
☐ 1930 to 1949
☐ 1950 to 1966
☐ 1967 to 1982
☐ 1983 to 2002
☐ 2003 or later
Listed building or conservation area?
☐ Yes     ☐ No
	PAS 2035:2023 says every domestic retrofit project is coordinated by a Retrofit Coordinator, and every dwelling is first assessed by a Retrofit Assessor. The assessment covers the construction and condition, defects, damp and mould, ventilation, heating and hot water, planning constraints and any measures already installed.



Walk Cam: retrofit assessment
Walk Cam video walk-through: available in the SiteSurvey app only.
2. Fabric and condition
Main walls  (choose one)
☐ Solid brick
☐ Cavity, unfilled
☐ Cavity, filled
☐ Timber frame
☐ System build
☐ Stone
Loft insulation depth (mm)
______________________________________________________________________________
Ground floor  (choose one)
☐ Suspended timber     ☐ Solid     ☐ Unknown
Glazing  (choose one)
☐ Single     ☐ Double before 2002     ☐ Double 2002 or later     ☐ Triple     ☐ Mixed
Defects to fix before retrofit  (tick all that apply)
☐ Damp or mould
☐ Roof leaks
☐ Gutters or downpipes
☐ Cracked render or pointing
☐ High ground levels
☐ Blocked air bricks
☐ None found
	If applicable: PAS 2035 asks for structural defects to be repaired and the causes of damp or water ingress to be dealt with before retrofit measures are installed.



Photos of defects  (photos: attach, or note the file names)
______________________________________________________________________________
3. Ventilation, heating and occupancy
Ventilation *  (tick all that apply)
☐ Trickle vents
☐ Kitchen extract
☐ Bathroom extract
☐ Continuous (dMEV)
☐ Positive input ventilation (PIV)
☐ MVHR
☐ None
Do the extract fans run and move air?  (choose one)
☐ Yes     ☐ No, or weak     ☐ No fans fitted
Main heating  (choose one)
☐ Gas boiler
☐ Oil boiler
☐ Electric storage
☐ Heat pump
☐ Solid fuel
☐ Other
Boiler make, model and age
______________________________________________________________________________
Occupants
______________________________________________________________________________
Occupancy and comfort notes (cold rooms, condensation, health)
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
Improvement options noted
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
Householder name
______________________________________________________________________________
Householder signature
	



Completed by *
______________________________________________________________________________
Signature
	



Retrofit Assessment Record. Printable copy from the SiteSurvey form library. Fill it in on a phone, with photos and signatures: sitesurvey.app/forms/retrofit-assessment-template/




