Roof Survey and Measure
A roof survey and measure for quoting: each slope with its covering, eaves and rafter lengths, area and pitch, ridges, hips, valleys and rainwater goods, access, fragile surfaces and asbestos.
1. Property and access
Project
______________________________________________________________________________
Client
______________________________________________________________________________
Site *
______________________________________________________________________________
Site address
______________________________________________________________________________
Survey date *
______________________________________________________________________________
Time
______________________________________________________________________________
Surveyed by *
______________________________________________________________________________
Roof type  (choose one)
☐ Pitched     ☐ Flat     ☐ Mixed pitched and flat     ☐ Mansard     ☐ Other
Age of the property  (choose one)
☐ Before 1919
☐ 1919 to 1944
☐ 1945 to 1979
☐ 1980 to 1999
☐ 2000 or later
☐ Not known
Access needed  (tick all that apply)
☐ Scaffold
☐ Tower
☐ MEWP
☐ Roof ladder
☐ Edge protection
☐ Other: ____________
Are there fragile surfaces, such as rooflights or sheeted roofs?
☐ Yes     ☐ No
	If applicable: HSE: the main causes of death and injury in roof work are falls from roof edges or openings and through fragile roofs and rooflights. Treat all roofs as fragile until a competent person has confirmed they are not. The Work at Height Regulations 2005, regulation 9, require steps to prevent anyone falling through a fragile surface: no passing across or near, or working on or near, a fragile surface where it is reasonably practicable to work safely another way; otherwise suitable platforms, coverings, guard rails or other means, and warning notices at the approach. HSE guidance HSG33, Health and safety in roof work, sets out how.



Could any material contain asbestos (for example cement sheets or tiles, soffits or undercloaks)?
☐ Yes     ☐ No
	If applicable: HSE: asbestos can be present in any building built or refurbished before 2000, including asbestos cement roof sheets and tiles, soffits and undercloaks. Have suspect materials checked before quoting work that disturbs them.



Walk Cam: roof survey
Walk Cam video walk-through: available in the SiteSurvey app only.
Weather capture
Digital form: use Record current conditions. On paper, record date/time, temperature (°C), wind (mph and direction), conditions and source. Keep observed conditions separate from forecast estimates.
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
2. Slopes and areas
Roof slopes or flat areas  (copy this block for each one)
Slope reference *
______________________________________________________________________________
Covering  (choose one)
☐ Concrete tiles
☐ Clay tiles
☐ Slate
☐ Fibre cement slate
☐ Felt
☐ EPDM
☐ GRP
☐ Metal sheet
☐ Other
Eaves length (m) *
Measuring from a photo gives an estimate. Check key lengths with a tape before ordering.
______________________________________________________________________________
Length along the top edge (m) *
The ridge or top edge of this slope. The same as the eaves for a rectangular slope, 0 for a triangular hip end.
______________________________________________________________________________
Rafter length, eaves to ridge, measured up the slope (m) *
Measuring from a photo gives an estimate. Check key lengths with a tape before ordering.
______________________________________________________________________________
Slope area (m²)  (if applicable; worked out automatically in the app)
______________________________________________________________________________
Pitch (degrees)
______________________________________________________________________________
Condition  (choose one)
☐ Good     ☐ Fair     ☐ Poor     ☐ Failed
Defects
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
Photos  (photos: attach, or note the file names)
______________________________________________________________________________
Total roof area (m²)  (worked out automatically in the app)
______________________________________________________________________________
3. Ridges, valleys and rainwater
Ridge (m)
Measuring from a photo gives an estimate. Check key lengths with a tape before ordering.
______________________________________________________________________________
Hips (m)
Measuring from a photo gives an estimate. Check key lengths with a tape before ordering.
______________________________________________________________________________
Valleys (m)
Measuring from a photo gives an estimate. Check key lengths with a tape before ordering.
______________________________________________________________________________
Verges (m)
Measuring from a photo gives an estimate. Check key lengths with a tape before ordering.
______________________________________________________________________________
Abutment flashings (m)
Measuring from a photo gives an estimate. Check key lengths with a tape before ordering.
______________________________________________________________________________
Gutters (m)
Measuring from a photo gives an estimate. Check key lengths with a tape before ordering.
______________________________________________________________________________
Downpipes (m)
Measuring from a photo gives an estimate. Check key lengths with a tape before ordering.
______________________________________________________________________________
Chimney stacks
______________________________________________________________________________
Rooflights
______________________________________________________________________________
Fascias, soffits and bargeboards
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
Work recommended
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
4. Actions and sign-off
Are further actions needed?
☐ Yes     ☐ No
Further actions  (copy this block for each one; if applicable)
What needs doing? *
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
Priority  (choose one)
☐ Urgent     ☐ High     ☐ Medium     ☐ Low
Who will do it?
______________________________________________________________________________
Due date
______________________________________________________________________________
Status  (choose one)
☐ Open     ☐ In progress     ☐ Completed
Inspector name *
______________________________________________________________________________
Position or company
______________________________________________________________________________
Inspector signature
	



	Signing records what was found on the day. It does not make unsafe equipment safe or replace a thorough examination, design check or service by a competent person.



Roof Survey and Measure. Printable copy from the SiteSurvey form library. Fill it in on a phone, with photos and signatures: sitesurvey.app/forms/roof-measurement-survey-template/




