Window and Door Survey
A window and door survey: each opening with its room, elevation, measurements, existing and new style, glazing, safety glass, escape window sizes and trickle vents, plus photos inside and out.
1. Property
Project
______________________________________________________________________________
Client
______________________________________________________________________________
Site *
______________________________________________________________________________
Site address
______________________________________________________________________________
Survey date *
______________________________________________________________________________
Time
______________________________________________________________________________
Surveyed by *
______________________________________________________________________________
Property type  (choose one)
☐ Detached house
☐ Semi-detached house
☐ Terraced house
☐ Bungalow
☐ Flat
☐ Commercial building
☐ Other
Age of the property  (choose one)
☐ Before 1919
☐ 1919 to 1944
☐ 1945 to 1979
☐ 1980 to 1999
☐ 2000 or later
☐ Not known
Is the building listed or in a conservation area?
☐ Yes     ☐ No
	If applicable: Listed buildings and conservation areas often need consent for new windows or doors. Check with the local planning authority before ordering.



	Building Regulations (England). Approved Document L sets a limiting U-value of 1.4 W/m²K, or Window Energy Rating band B, for replacement windows in existing homes. Approved Document B says the work should comply with Parts K and L and leave the building no worse than before for means of escape, and Approved Document F says ventilation should be no worse than before. Installers registered with a competent person scheme such as FENSA or Certass can self-certify the work, so building control does not need to be told separately.



Walk Cam: window and door survey
Walk Cam video walk-through: available in the SiteSurvey app only.
2. Windows and doors
Openings  (copy this block for each one)
Reference (for example W1 or D1) *
______________________________________________________________________________
Room *
______________________________________________________________________________
Elevation  (choose one)
☐ Front     ☐ Rear     ☐ Left side     ☐ Right side
Opening *  (choose one)
☐ Window     ☐ Door     ☐ Patio, French or bifold door     ☐ Roof window
Existing frame material  (choose one)
☐ uPVC     ☐ Timber     ☐ Aluminium     ☐ Steel     ☐ Composite
Existing condition  (choose one)
☐ Good     ☐ Fair     ☐ Poor     ☐ Failed
Measured as  (choose one)
☐ Structural opening (brick to brick)
☐ Existing frame size
☐ Finished size to order
Width (mm) *
______________________________________________________________________________
Height (mm) *
______________________________________________________________________________
New style  (choose one)
☐ Casement
☐ Tilt and turn
☐ Sliding sash
☐ Fixed
☐ Bay
☐ Bow
☐ Composite door
☐ French doors
☐ Bifold doors
☐ Sliding patio door
☐ Roof window
New frame material  (choose one)
☐ uPVC     ☐ Aluminium     ☐ Timber     ☐ Composite
Colour inside and outside
______________________________________________________________________________
Glazing  (choose one)
☐ Double     ☐ Triple
Obscure glass needed?
☐ Yes     ☐ No
Is any glazing within 800 mm of the floor, or within 1500 mm of the floor in a door or in a side panel within 300 mm of a door?
☐ Yes     ☐ No
	If applicable: Critical location. Approved Document K says glazing here should break safely (safety glazing tested to BS EN 12600), resist impact without breaking, be in small panes, or be permanently protected.



Must this window provide an escape route (for example a habitable room on the first floor)?  (if applicable)
☐ Yes     ☐ No
Clear opening width when open (mm)  (if applicable)
______________________________________________________________________________
Clear opening height when open (mm)  (if applicable)
______________________________________________________________________________
Floor to bottom of the opening (mm)  (if applicable)
______________________________________________________________________________
Clear opening area (m²)  (if applicable; worked out automatically in the app)
______________________________________________________________________________
	If applicable: Below the escape window size in Approved Document B: an unobstructed openable area of at least 0.33 m², at least 450 mm wide and 450 mm high, with the bottom no more than 1100 mm above the floor. A replacement for a window big enough for escape should give at least the same potential for escape, or at least this minimum if the old one was larger.



Does the existing window have trickle vents?  (if applicable)
☐ Yes     ☐ No
	If applicable: Approved Document F: the replacement should have trickle vents (background ventilators) no smaller than the existing ones, controllable by the occupant or automatically.



	If applicable: Approved Document F: replacing windows makes a home more airtight, so ventilation must be no worse than before. One way is trickle vents in the new windows of at least 8000 mm² equivalent area in habitable rooms and kitchens, and 4000 mm² in bathrooms.



Cill, internal finish and making good
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
Photo from inside  (photos: attach, or note the file names)
______________________________________________________________________________
Photo from outside  (photos: attach, or note the file names)
______________________________________________________________________________
3. Access and fitting
Access needed  (tick all that apply)
☐ Ladder     ☐ Tower     ☐ Scaffold     ☐ None     ☐ Other: ____________
Is there parking for the fitting van?
☐ Yes     ☐ No
Things to plan for  (tick all that apply)
☐ Furniture to move
☐ Blinds or curtains to remove
☐ Alarm contacts on frames
☐ Possible asbestos panels
☐ Narrow access
☐ None
Notes for the fitters
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
4. Actions and sign-off
Are further actions needed?
☐ Yes     ☐ No
Further actions  (copy this block for each one; if applicable)
What needs doing? *
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
Who will do it?
______________________________________________________________________________
Due date
______________________________________________________________________________
Status  (choose one)
☐ Open     ☐ In progress     ☐ Completed
Inspector name *
______________________________________________________________________________
Position or company
______________________________________________________________________________
Inspector signature
	



	Signing records what was found on the day. It does not make unsafe equipment safe or replace a thorough examination, design check or service by a competent person.



Window and Door Survey. Printable copy from the SiteSurvey form library. Fill it in on a phone, with photos and signatures: sitesurvey.app/forms/window-survey-template/




