Automatic Door Service Record
An automatic door and gate service record: each door with type and label scan, activation and safety sensors, obstruction stop, manual opening on power failure, emergency break-out, signage, result and recommendations.
1. Visit
Project
______________________________________________________________________________
Client
______________________________________________________________________________
Site *
______________________________________________________________________________
Site address
______________________________________________________________________________
Service date *
______________________________________________________________________________
Time
______________________________________________________________________________
Engineer *
______________________________________________________________________________
Company
______________________________________________________________________________
	Workplace (Health, Safety and Welfare) Regulations 1992, regulation 18: a powered door or gate must have suitable and effective features to prevent it causing injury by trapping anyone, and where needed for health or safety it must be possible to open it by hand unless it opens automatically if the power fails. HSE's Approved Code of Practice (L24) gives examples: a sensitive edge or other detector that stops or reverses the door when obstructed, and a device that limits the closing force.



2. Doors and gates
Doors  (copy this block for each one)
Location *
______________________________________________________________________________
Type  (choose one)
☐ Sliding door
☐ Swing door
☐ Revolving door
☐ Folding door
☐ Sliding gate
☐ Swing gate
☐ Barrier
Scan the operator label
Scanned in the SiteSurvey app. On paper, write the numbers: serial number, model number.
______________________________________________________________________________
______________________________________________________________________________
Activation sensors and controls  (choose one)
☐ OK     ☐ Defect
Safety sensors stop or reverse the door on an obstruction  (choose one)
☐ OK     ☐ Defect
Closing force and speed within limits  (choose one)
☐ OK     ☐ Defect
Closing force measured with a force meter?
☐ Yes     ☐ No
Opens by hand on power failure, or opens automatically  (choose one)
☐ OK     ☐ Defect
Emergency break-out or escape function  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
Signs and markings  (choose one)
☐ OK     ☐ Defect
Result *  (choose one)
☐ Safe     ☐ Safe with recommendations     ☐ Unsafe: taken out of service
Defects and recommendations  (if applicable)
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
	If applicable: Unsafe. Leave it out of service and tell the site contact in writing.



Who was told it is out of service, and when  (if applicable)
______________________________________________________________________________
Photos  (photos: attach, or note the file names)
______________________________________________________________________________
Doors taken out of service  (worked out automatically in the app)
______________________________________________________________________________
Doors with recommendations  (worked out automatically in the app)
______________________________________________________________________________
3. Sign-off
Site contact name
______________________________________________________________________________
Site contact signature
	



Completed by *
______________________________________________________________________________
Signature
	



Automatic Door Service Record. Printable copy from the SiteSurvey form library. Fill it in on a phone, with photos and signatures: sitesurvey.app/forms/automatic-door-maintenance-checklist/




