Dock Leveller and Loading Bay Inspection
A dock leveller and loading bay inspection: each bay's leveller, lip, hydraulics, toe guards, dock shelter and door, vehicle restraint or chocks, lights and signals, bumpers, markings, result and photos.
1. Site
Project
______________________________________________________________________________
Client
______________________________________________________________________________
Site *
______________________________________________________________________________
Site address
______________________________________________________________________________
Inspection date *
______________________________________________________________________________
Time
______________________________________________________________________________
Inspector *
______________________________________________________________________________
Last engineer service of the levellers
______________________________________________________________________________
	HSE HSG76: a vehicle moving before loading or unloading is finished (a driveaway) can cause serious accidents, so there must be a safe system of work, such as vehicle restraints, interlocks, key control or traffic lights. Dock levellers need toe guards, skirts to enclose trapping points, planned routine maintenance and a system to report and repair defects.



2. Bays
Bays  (copy this block for each one)
Bay number *
______________________________________________________________________________
Leveller deck and lip  (choose one)
☐ OK     ☐ Defect
Hydraulics, no leaks  (choose one)
☐ OK     ☐ Defect
Toe guards and side skirts  (choose one)
☐ OK     ☐ Defect
Dock door and shelter  (choose one)
☐ OK     ☐ Defect
Vehicle restraint, chocks or interlock  (choose one)
☐ OK     ☐ Defect     ☐ None fitted
Traffic lights and signals  (choose one)
☐ OK     ☐ Defect     ☐ None fitted
Dock bumpers  (choose one)
☐ OK     ☐ Defect
Markings and edge protection  (choose one)
☐ OK     ☐ Defect
Result *  (choose one)
☐ Safe to use     ☐ Use with care: repair booked     ☐ Out of use
Defects  (if applicable)
______________________________________________________________________________
Photos  (photos: attach, or note the file names)
______________________________________________________________________________
Bays out of use  (worked out automatically in the app)
______________________________________________________________________________
Bays with no vehicle restraint  (worked out automatically in the app)
______________________________________________________________________________
3. Actions and sign-off
Are further actions needed?
☐ Yes     ☐ No
Further actions  (copy this block for each one; if applicable)
What needs doing? *
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
Who will do it?
______________________________________________________________________________
Due date
______________________________________________________________________________
Status  (choose one)
☐ Open     ☐ In progress     ☐ Completed
Inspector name *
______________________________________________________________________________
Position or company
______________________________________________________________________________
Inspector signature
	



	Signing records what was found on the day. It does not make unsafe equipment safe or replace a thorough examination, design check or service by a competent person.



Dock Leveller and Loading Bay Inspection. Printable copy from the SiteSurvey form library. Fill it in on a phone, with photos and signatures: sitesurvey.app/forms/dock-leveller-inspection/




