Fence and Boundary Inspection
A fence and boundary inspection: what the boundary is for, each section with its type, posts, panels, gaps and climbing aids, gates with hinges, latches and locks, breaches made safe, photos and repair actions.
1. Site
Project
______________________________________________________________________________
Client
______________________________________________________________________________
Site *
______________________________________________________________________________
Site address
______________________________________________________________________________
Inspection date *
______________________________________________________________________________
Time
______________________________________________________________________________
Inspector *
______________________________________________________________________________
Reason for the inspection  (choose one)
☐ Routine     ☐ After a storm     ☐ After a report of damage or a break-in
What the boundary is for  (tick all that apply)
☐ Security
☐ Keeping the public or children out
☐ Keeping animals in
☐ Privacy
☐ Marking the legal boundary
Is this a construction site perimeter?
☐ Yes     ☐ No
	If applicable: HSE: construction sites need measures to manage access across defined boundaries and steps to exclude unauthorised people. Plan the perimeter, provide the fencing and maintain it. HSE says that in populated areas this will typically mean a two-metre high small mesh fence or hoarding.



Does a public right of way cross or run alongside the boundary?
☐ Yes     ☐ No
	If applicable: Leeds City Council's guidance for landowners: gates and stiles on rights of way are the landowner's to maintain, barbed wire must not be strung across a right of way, and the council's consent is needed before an electric fence is put across one. Check your own council's rules.



	Under section 2 of the Occupiers' Liability Act 1957, an occupier must take such care as is reasonable to see that visitors will be reasonably safe, and must be prepared for children to be less careful than adults. A dated record shows what was checked and done.



Weather capture
Digital form: use Record current conditions. On paper, record date/time, temperature (°C), wind (mph and direction), conditions and source. Keep observed conditions separate from forecast estimates.
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
2. Boundary
Start point (a gate or corner you can find again)
______________________________________________________________________________
Height the fence needs to be (m)
Optional. From the site plan, the client's specification or your security risk assessment. The form compares each section with it.
______________________________________________________________________________
Fence sections  (copy this block for each one)
Section (from, to) *
______________________________________________________________________________
Type  (choose one)
☐ Timber panel
☐ Close board
☐ Post and rail
☐ Chain link
☐ Weldmesh or palisade
☐ Temporary mesh panels
☐ Hoarding
☐ Wall
☐ Hedge
Start and end of the section (GPS)
Optional. Mark both ends, so the repair team finds the section.
______________________________________________________________________________
Length (m)
By tape, pacing or the site plan.
______________________________________________________________________________
Height (m)
Optional. Use a tape, or measure from a photo taken square on with something of known size in the same plane, such as a standard 1.83 m (6 ft) panel width.
______________________________________________________________________________
Against the height needed  (if applicable; worked out automatically in the app)
______________________________________________________________________________
Posts upright and firm  (choose one)
☐ OK     ☐ Defect
Panels, rails or mesh intact  (choose one)
☐ OK     ☐ Defect
No gaps under or through  (choose one)
☐ OK     ☐ Defect
Nothing next to it that helps people climb over  (choose one)
☐ OK     ☐ Defect
Barbed or razor wire  (choose one)
☐ None fitted     ☐ OK     ☐ Damaged or loose
Result *  (choose one)
☐ OK     ☐ Repair needed     ☐ Breach: made safe
What is wrong?  (if applicable)
______________________________________________________________________________
How the breach was made safe  (if applicable)
______________________________________________________________________________
Photos  (photos: attach, or note the file names)
______________________________________________________________________________
is_low  (worked out automatically in the app)
______________________________________________________________________________
len_bad  (worked out automatically in the app)
______________________________________________________________________________
Total length walked (m)  (worked out automatically in the app)
______________________________________________________________________________
Sections  (worked out automatically in the app)
______________________________________________________________________________
Length needing repair or breached (m)  (worked out automatically in the app)
______________________________________________________________________________
Share of the length walked (%)  (if applicable; worked out automatically in the app)
______________________________________________________________________________
Sections needing repair  (worked out automatically in the app)
______________________________________________________________________________
Breaches  (worked out automatically in the app)
______________________________________________________________________________
Sections lower than needed  (if applicable; worked out automatically in the app)
______________________________________________________________________________
	If applicable: A breach was made safe temporarily. Set the permanent repair as an action with an owner and a date, and recheck the temporary fix until it is done.



Are there gates on this boundary?
☐ Yes     ☐ No
Gates  (copy this block for each one; if applicable)
Gate *
______________________________________________________________________________
Hinges and posts  (choose one)
☐ OK     ☐ Defect
Closes and stays shut  (choose one)
☐ OK     ☐ Defect
Lock or padlock  (choose one)
☐ OK     ☐ Defect     ☐ None fitted
What is wrong?  (if applicable)
______________________________________________________________________________
Photos  (photos: attach, or note the file names)
______________________________________________________________________________
g_bad  (worked out automatically in the app)
______________________________________________________________________________
Gates checked  (if applicable; worked out automatically in the app)
______________________________________________________________________________
Gates with a defect  (if applicable; worked out automatically in the app)
______________________________________________________________________________
Walk Cam: fence and boundary inspection
Walk Cam video walk-through: available in the SiteSurvey app only.
3. Actions and sign-off
Are further actions needed?
☐ Yes     ☐ No
Further actions  (copy this block for each one; if applicable)
What needs doing? *
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
Priority  (choose one)
☐ Urgent     ☐ High     ☐ Medium     ☐ Low
Who will do it?
______________________________________________________________________________
Due date
______________________________________________________________________________
Status  (choose one)
☐ Open     ☐ In progress     ☐ Completed
Actions open or in progress  (if applicable; worked out automatically in the app)
______________________________________________________________________________
Next inspection due
Set by the owner's own inspection regime. Also inspect after storms and reports of damage.
______________________________________________________________________________
Days until the next inspection  (if applicable; worked out automatically in the app)
______________________________________________________________________________
	If applicable: Check the date. The next date is before the date of this visit.



Inspector name *
______________________________________________________________________________
Position or company
______________________________________________________________________________
Inspector signature
	



	Signing records what was found on the day. It does not make unsafe equipment safe or replace a thorough examination, design check or service by a competent person.



Fence and Boundary Inspection. Printable copy from the SiteSurvey form library. Fill it in on a phone, with photos and signatures: sitesurvey.app/forms/fence-inspection-checklist/




