Fire Stopping Installation Record
A fire stopping installation record: certification scheme, drawings, each penetration seal with its label, element, fire rating, services, product and tested detail, before and after photos, and sign-off.
1. Job
Project
______________________________________________________________________________
Client
______________________________________________________________________________
Site *
______________________________________________________________________________
Site address
______________________________________________________________________________
Date *
______________________________________________________________________________
Time
______________________________________________________________________________
Installer *
______________________________________________________________________________
Operatives (names and qualification or card)
______________________________________________________________________________
Third-party certification scheme  (choose one)
☐ FIRAS     ☐ LPCB     ☐ IFC     ☐ BM TRADA     ☐ Other     ☐ None
Certificate number
______________________________________________________________________________
	ASFP on-site guide to installing fire-stopping: fire stopping should ideally be installed by competent persons, meaning people working for a third-party certificated contractor or whose competence a third-party scheme has checked. Make a complete record of all installations, referred to in the labelling, apply labels for traceability, and photograph the completed work.



	If applicable: No third-party certification recorded. The ASFP recommends installation by a third-party certificated contractor or by people whose competence a third-party scheme has checked.



	Approved Document B (England): openings through a fire-resisting element for pipes, ducts, conduits or cables should be as few as possible, as small as practicable and fire-stopped, and joints between fire-separating elements should be fire-stopped.



Drawings or fire strategy reference
______________________________________________________________________________
Level or area
______________________________________________________________________________
2. Penetrations sealed
Seals  (copy this block for each one)
Label or reference number *
______________________________________________________________________________
Scan the seal label
Scanned in the SiteSurvey app. On paper, write the numbers: label number.
______________________________________________________________________________
Location
______________________________________________________________________________
Element  (choose one)
☐ Wall     ☐ Floor     ☐ Ceiling or cavity barrier
Fire resistance  (choose one)
☐ 30 minutes     ☐ 60 minutes     ☐ 90 minutes     ☐ 120 minutes     ☐ Other
Services through it  (tick all that apply)
☐ Cables
☐ Plastic pipe
☐ Metal pipe
☐ Insulated pipe
☐ Ductwork
☐ Mixed services
☐ Linear gap
Product or system
______________________________________________________________________________
Tested detail or assessment reference
______________________________________________________________________________
Before photo  (photos: attach, or note the file names)
______________________________________________________________________________
After photo (with label)  (photos: attach, or note the file names)
______________________________________________________________________________
Result *  (choose one)
☐ Complete     ☐ Snag     ☐ Outside the tested detail: needs assessment
What is needed  (if applicable)
______________________________________________________________________________
Seals complete  (worked out automatically in the app)
______________________________________________________________________________
Seals with snags  (worked out automatically in the app)
______________________________________________________________________________
Seals needing assessment  (worked out automatically in the app)
______________________________________________________________________________
	Photograph each seal before it is covered up, and again once it is labelled, so the work can be checked later.



3. Sign-off
Notes for the main contractor
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
Main contractor or client name
______________________________________________________________________________
Main contractor or client signature
	



Completed by *
______________________________________________________________________________
Signature
	



Fire Stopping Installation Record. Printable copy from the SiteSurvey form library. Fill it in on a phone, with photos and signatures: sitesurvey.app/forms/fire-stopping-installation-record/




