Floor Moisture and Pre-install Survey
A floor moisture and pre-installation survey: base type and age, conditions, relative humidity readings with a hygrometer hood, flatness, damp-proof membrane, the manufacturer's limit and whether flooring can go down.
1. Base
Project
______________________________________________________________________________
Client
______________________________________________________________________________
Site *
______________________________________________________________________________
Site address
______________________________________________________________________________
Survey date *
______________________________________________________________________________
Time
______________________________________________________________________________
Surveyor *
______________________________________________________________________________
Base  (choose one)
☐ Sand and cement screed
☐ Concrete slab
☐ Calcium sulphate (anhydrite) screed
☐ Timber or board
☐ Existing floor covering
Age of the base (weeks)
______________________________________________________________________________
Floor covering to be laid *
______________________________________________________________________________
Manufacturer's maximum relative humidity (%)
From the adhesive and floor covering manufacturers' data. Use the lower figure.
______________________________________________________________________________
Was the building at its normal service temperature and humidity, with drying equipment off, before the readings were taken?
☐ Yes     ☐ No
	If applicable: Readings taken while drying equipment is running may not show how wet the base will be in normal use. Say so under preparation.



Weather capture
Digital form: use Record current conditions. On paper, record date/time, temperature (°C), wind (mph and direction), conditions and source. Keep observed conditions separate from forecast estimates.
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
2. Readings
Readings  (copy this block for each one)
Location *
______________________________________________________________________________
Method  (choose one)
☐ Hygrometer hood (RH %)     ☐ Moisture meter (comparative)     ☐ Carbide or oven test
Relative humidity (%)  (if applicable)
______________________________________________________________________________
Meter reading and scale  (if applicable)
______________________________________________________________________________
Moisture content (%)  (if applicable)
______________________________________________________________________________
Temperature (°C)
______________________________________________________________________________
Hood in place for (hours)  (if applicable)
Hood makers and BS 8203 practice: leave the sealed hood for at least 72 hours, then read until the value is stable, or as the hood maker states.
______________________________________________________________________________
	If applicable: The hood has been in place for less than 72 hours. The reading may not have reached equilibrium yet.



Difference from the limit (% RH, above 0 is too wet)  (if applicable; worked out automatically in the app)
______________________________________________________________________________
	If applicable: Above the manufacturer's limit. Do not lay the floor covering yet.



Photos  (photos: attach, or note the file names)
______________________________________________________________________________
Readings taken  (worked out automatically in the app)
______________________________________________________________________________
Hygrometer readings  (worked out automatically in the app)
______________________________________________________________________________
Highest relative humidity (%)  (worked out automatically in the app)
______________________________________________________________________________
Readings over the limit  (if applicable; worked out automatically in the app)
______________________________________________________________________________
Readings within the limit  (if applicable; worked out automatically in the app)
______________________________________________________________________________
Relative humidity result  (if applicable; worked out automatically in the app)
______________________________________________________________________________
	Compare each relative humidity reading with the lowest limit given by the adhesive and floor covering manufacturers. BS 8203 is the code of practice for installing resilient floor coverings, and BS 8204-1 covers concrete bases and levelling screeds that receive them.



3. Flatness and result
Worst gap under a 2 m straightedge (mm)
______________________________________________________________________________
Flatness limit from the specification (mm)
The largest gap the specification or the covering manufacturer allows under the straightedge.
______________________________________________________________________________
Flatness check  (if applicable; worked out automatically in the app)
______________________________________________________________________________
	If applicable: The gap is larger than the specification allows. Record the smoothing or grinding needed before the covering goes down.



Damp-proof membrane present?
☐ Yes     ☐ No
Result *  (choose one)
☐ Ready to lay
☐ Ready after preparation
☐ Not ready: too wet
☐ Not ready: other
Preparation needed (smoothing, priming, surface DPM, drying time)  (if applicable)
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
Client or main contractor name
______________________________________________________________________________
Client or main contractor signature
	



Completed by *
______________________________________________________________________________
Signature
	



Floor Moisture and Pre-install Survey. Printable copy from the SiteSurvey form library. Fill it in on a phone, with photos and signatures: sitesurvey.app/forms/floor-moisture-test-record/




