Gutter Clearance Report
A gutter clearance report with before and after photos: access method, each elevation's length and blockage, downpipes flushed, defects found, recommendations and the customer's signature.
1. Job
Project
______________________________________________________________________________
Client
______________________________________________________________________________
Site *
______________________________________________________________________________
Site address
______________________________________________________________________________
Property location
Mark it at the front of the property, as a record of the visit. Tap Mark current location on site. It saves the coordinates, a grid reference and the accuracy.
______________________________________________________________________________
Date *
______________________________________________________________________________
Time
______________________________________________________________________________
Operative *
______________________________________________________________________________
Access *  (tick all that apply)
☐ Gutter vacuum from the ground     ☐ Ladder     ☐ Tower     ☐ MEWP     ☐ Roof access
	If applicable: HSE: avoid work at height where it is reasonably practicable, and do as much of the work as possible from the ground. Where it cannot be avoided, use the right equipment. Use ladders only for light work of short duration (HSE says a maximum of 30 minutes at a time), and do not rest a ladder against weak surfaces such as plastic gutters.



Weather capture
Digital form: use Record current conditions. On paper, record date/time, temperature (°C), wind (mph and direction), conditions and source. Keep observed conditions separate from forecast estimates.
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
2. Gutters
Elevations or runs  (copy this block for each one)
Elevation or run (for example front, rear, garage) *
______________________________________________________________________________
Length (m)
______________________________________________________________________________
Height to the gutter (m)
Measure from a square-on photo of the elevation with the front door as the reference, to plan access and price the next visit. Measuring from a photo gives an estimate.
______________________________________________________________________________
Blockage  (choose one)
☐ Clear     ☐ Partly blocked     ☐ Fully blocked
Before photos  (photos: attach, or note the file names)
______________________________________________________________________________
After photos  (photos: attach, or note the file names)
______________________________________________________________________________
Downpipes flushed and running?
☐ Yes     ☐ No
Damage found on this run
______________________________________________________________________________
Total gutter cleared (m)  (worked out automatically in the app)
______________________________________________________________________________
Runs fully blocked  (worked out automatically in the app)
______________________________________________________________________________
Runs cleared  (worked out automatically in the app)
______________________________________________________________________________
Runs partly blocked  (worked out automatically in the app)
______________________________________________________________________________
Runs where the downpipes did not run clear  (worked out automatically in the app)
______________________________________________________________________________
Highest gutter (m)  (worked out automatically in the app)
______________________________________________________________________________
Defects found  (tick all that apply)
☐ Leaking joints
☐ Sagging or broken brackets
☐ Cracked sections
☐ Plants growing
☐ Fascia or soffit damage
☐ Overflowing downpipe
☐ None found
Defects to fix  (copy this block for each one; if applicable)
Defect and where *
______________________________________________________________________________
Photos  (photos: attach, or note the file names)
______________________________________________________________________________
Priority  (choose one)
☐ Urgent     ☐ High     ☐ Medium     ☐ Low
Recommendations and quote
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
Recommended next clearance
Set from the build-up found and nearby trees.
______________________________________________________________________________
Walk Cam: gutter condition visual inspection
Walk Cam video walk-through: available in the SiteSurvey app only.
3. Sign-off
Customer name
______________________________________________________________________________
Customer signature
	



Completed by *
______________________________________________________________________________
Signature
	



Gutter Clearance Report. Printable copy from the SiteSurvey form library. Fill it in on a phone, with photos and signatures: sitesurvey.app/forms/gutter-clearance-report/




