Landlord Electrical Visual Check
A landlord's electrical visual check between EICRs: the last EICR date and code, sockets, switches, lights, consumer unit, RCD test, flexes, bathroom and outside fittings, photos and actions.
1. Property
Project
______________________________________________________________________________
Client
______________________________________________________________________________
Site *
______________________________________________________________________________
Site address
______________________________________________________________________________
Date *
______________________________________________________________________________
Time
______________________________________________________________________________
Checked by *
______________________________________________________________________________
Reason  (choose one)
☐ Change of tenancy     ☐ Routine check     ☐ Tenant reported a problem
Date of the last EICR
______________________________________________________________________________
Days since the EICR  (if applicable; worked out automatically in the app)
______________________________________________________________________________
	If applicable: More than 5 years since the EICR. The Electrical Safety Standards regulations require landlords in England to have the installation inspected and tested by a qualified person at least every 5 years, or sooner if the report says so.



Next inspection due (date given on the EICR)
______________________________________________________________________________
	If applicable: The next inspection date on the EICR has passed. Book an inspection and test.



Last EICR result  (choose one)
☐ Satisfactory     ☐ Unsatisfactory, remedial work done     ☐ Not known
Has the tenant been given a copy of the current EICR?
☐ Yes     ☐ No
	If applicable: The landlord must give a copy of the report to a new tenant before they move in, and to an existing tenant within 28 days of the inspection.



	A visual check does not replace an EICR. GOV.UK guidance recommends at least a visual inspection before a new tenancy starts, to confirm nothing has been damaged since the last report. Anything that looks unsafe goes to a qualified electrician.



2. Checks
Sockets and switches: no damage, scorch marks or loose fittings  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
Light fittings and ceiling roses undamaged  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
Consumer unit: cover on, no damage, labels legible  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
RCD test button trips and resets  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
Meter and supply intake: no damage or signs of burning  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
No taped repairs, damaged flexes or overloaded adaptors  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
Bathroom: no sockets within 2.5 m of the bath or shower (shaver sockets excepted), fittings undamaged  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
Outside lights and sockets undamaged and covered  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
Landlord's appliances undamaged (cooker, extractor, heaters)  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
Photos of any problems  (photos: attach, or note the file names)
______________________________________________________________________________
Is anything dangerous now (exposed live parts, burning smell, scorching)?
☐ Yes     ☐ No
	If applicable: Isolate the circuit if safe to do so and get a qualified electrician straight away.



3. Actions and sign-off
Are further actions needed?
☐ Yes     ☐ No
Further actions  (copy this block for each one; if applicable)
What needs doing? *
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
Who will do it?
______________________________________________________________________________
Due date
______________________________________________________________________________
Status  (choose one)
☐ Open     ☐ In progress     ☐ Completed
Inspector name *
______________________________________________________________________________
Position or company
______________________________________________________________________________
Inspector signature
	



	Signing records what was found on the day. It does not make unsafe equipment safe or replace a thorough examination, design check or service by a competent person.



Landlord Electrical Visual Check. Printable copy from the SiteSurvey form library. Fill it in on a phone, with photos and signatures: sitesurvey.app/forms/landlord-electrical-inspection-checklist/




