Landlord Gas Safety Record
A landlord gas safety site record: every appliance and flue with its checks, defects and remedial action, the installation checks, the engineer's Gas Safe number and the details regulation 36 requires.
1. Property and engineer
Project
______________________________________________________________________________
Client
______________________________________________________________________________
Site *
______________________________________________________________________________
Site address *
______________________________________________________________________________
Date of the check *
______________________________________________________________________________
Time
______________________________________________________________________________
Landlord or agent, name and address *
______________________________________________________________________________
Tenant
______________________________________________________________________________
Engineer name *
______________________________________________________________________________
Gas Safe registration number (business) *
______________________________________________________________________________
Engineer licence number
______________________________________________________________________________
	Gas Safety (Installation and Use) Regulations 1998, regulation 36. Landlords must have each appliance and flue checked for safety within 12 months of installation and then at least every 12 months, by a Gas Safe registered engineer. Give a copy of the record to existing tenants within 28 days of the check, and to new tenants before they move in. Keep it until two further checks have been made.



	This form records the information regulation 36 requires. Many engineers issue the formal record from their own certification software.



2. Appliances and flues
Appliances checked  (copy this block for each one)
Location *
______________________________________________________________________________
Type *  (choose one)
☐ Boiler
☐ Gas fire
☐ Cooker or hob
☐ Water heater
☐ Warm air heater
☐ Other
Make and model
______________________________________________________________________________
Scan the data plate
Scanned in the SiteSurvey app. On paper, write the numbers: serial number, model number.
______________________________________________________________________________
______________________________________________________________________________
Owned by the landlord?
☐ Yes     ☐ No
Flue type  (choose one)
☐ Room sealed     ☐ Open flue     ☐ Flueless     ☐ Balanced flue
Operating pressure or heat input
Or the combustion performance, where it is not reasonably practicable to examine these.
______________________________________________________________________________
Safety devices operate correctly  (choose one)
☐ Pass     ☐ Fail     ☐ Not applicable
Ventilation satisfactory  (choose one)
☐ Yes     ☐ No     ☐ Not applicable
Flue visual condition satisfactory  (choose one)
☐ Yes     ☐ No     ☐ Not applicable
Flue performance test (spillage or flue flow)  (choose one)
☐ Pass     ☐ Fail     ☐ Not applicable
Combustion analyser reading (CO ppm, CO/CO₂ ratio)
______________________________________________________________________________
Appliance serviced?
☐ Yes     ☐ No
Safe to use?
☐ Yes     ☐ No
Unsafe situation  (if applicable; choose one)
☐ At risk     ☐ Immediately dangerous
	If applicable: Unsafe appliance. Follow the Gas Industry Unsafe Situations Procedure, tell the responsible person, and record the warning label or notice issued.



Safety defect identified  (if applicable)
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
Remedial action taken  (if applicable)
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
Photos  (photos: attach, or note the file names)
______________________________________________________________________________
Appliances not safe to use  (worked out automatically in the app)
______________________________________________________________________________
3. Installation
Gas tightness test  (choose one)
☐ Pass     ☐ Fail     ☐ Not done
Emergency control valve accessible?
☐ Yes     ☐ No
Protective equipotential bonding present?
☐ Yes     ☐ No
Carbon monoxide alarm fitted in each room with a fixed combustion appliance (other than a gas cooker), and tested?
☐ Yes     ☐ No
	If applicable: In England, the Smoke and Carbon Monoxide Alarm (England) Regulations 2015 (as amended in 2022) require landlords to fit a carbon monoxide alarm in any room used as living accommodation that has a fixed combustion appliance, other than a gas cooker.



I confirm the check meets regulation 36(9) of the Gas Safety (Installation and Use) Regulations 1998 *
☐ Yes     ☐ No
Next check due by
Normally within 12 months of this check. If this check was done up to 2 months early under regulation 36A, the next is due 12 months from the original deadline.
______________________________________________________________________________
Engineer name *
______________________________________________________________________________
Engineer signature
	



Received by (landlord, agent or tenant)
______________________________________________________________________________
Signature
	



Landlord Gas Safety Record. Printable copy from the SiteSurvey form library. Fill it in on a phone, with photos and signatures: sitesurvey.app/forms/landlord-gas-safety-record-template/




