Vehicle Inspection Checklist
A daily vehicle inspection checklist and defect report for vans and cars: walkaround checks, mileage, tyre tread, photos of each side, defects graded safe or not to drive, and fleet sign-off.
1. Vehicle and driver
Project
______________________________________________________________________________
Client
______________________________________________________________________________
Depot or site
______________________________________________________________________________
Depot or site address
______________________________________________________________________________
Date of the check *
______________________________________________________________________________
Time
______________________________________________________________________________
Driver *
______________________________________________________________________________
Registration number *
______________________________________________________________________________
Scan the number plate or fleet tag
Scanned in the SiteSurvey app. On paper, write the numbers: registration, fleet number.
______________________________________________________________________________
______________________________________________________________________________
Vehicle  (choose one)
☐ Small van     ☐ Panel van (up to 3.5 tonnes)     ☐ Pickup     ☐ Car     ☐ Other
Make and model
______________________________________________________________________________
Odometer reading *
______________________________________________________________________________
Fuel or charge level  (choose one)
☐ Full     ☐ 3/4     ☐ 1/2     ☐ 1/4     ☐ Reserve
	DVSA van walkaround check. These are the 19 checks in the DVSA van drivers' daily walkaround check. Record the registration, the date, each defect, your assessment of it, your name and who you reported it to. Record nil defects if you find none. DVSA can ask for the record at a roadside check.



2. Walkaround checks
1. Front view, mirrors, cameras and glass: nothing blocking the view, windscreen not damaged  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
2. Windscreen washers and wipers work and are in good condition  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
3. Dashboard warning lights working, including ABS, airbag (SRS), EBS, EPS, ESC, full beam and parking brake  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
4. Steering moves properly, no excessive play  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
5. Horn works  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
6. Footwell clear; service brake and parking brake work without excessive travel  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
7. Seats secure; seat belts undamaged, latch and retract  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
8. Lights and indicators work; lenses fitted, clean and the right colour  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
9. Fluids, fuel and oil: levels correct, fuel filler cap secure, no leaks or puddles  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
10. Battery secure, in good condition, not leaking  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
11. Bodywork and doors: doors shut and secure, no sharp edges or loose panels  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
12. Tyres and wheels: legal tread, inflated, no deep cuts or visible cord, wheels secure  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
13. Load secure, right securing system, doors and tailgate lock  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
14. AdBlue (diesel exhaust fluid) topped up  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
15. Exhaust not leaking, no excessive smoke or noise  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
16. Alternative fuel system: isolation switch located, no leaks  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
17. Number plates correct, secure and readable  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
18. Tow bar and trailer secure, electrics working, breakaway cable fitted  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
19. Other equipment, such as a tail lift or other loading equipment, secure, undamaged and working  (choose one)
☐ OK     ☐ Defect     ☐ Not applicable
What is wrong?  (if applicable)
______________________________________________________________________________
Lowest tread depth measured (mm)
______________________________________________________________________________
	If applicable: Below the legal minimum. Cars and light vans need at least 1.6 mm of tread across the central three-quarters of the tread and around the whole circumference (Highway Code, annex 6). You can get 3 penalty points for each tyre that is not safe and legal. Do not drive the vehicle until the tyre is replaced.



Photos of the front, back and both sides  (photos: attach, or note the file names)
Four photos show the vehicle's condition at the start of the shift.
______________________________________________________________________________
3. Defects
Did you find any defects?
Answer No to record nil defects.
☐ Yes     ☐ No
Defects  (copy this block for each one; if applicable)
What is the defect and where? *
______________________________________________________________________________
Can the vehicle be driven? *  (choose one)
☐ Minor: safe to drive, report for repair     ☐ Dangerous: do not drive
	If applicable: Do not drive. DVSA says dangerous defects must be fixed before the journey continues. Tell your supervisor or fleet manager now.



Photos  (photos: attach, or note the file names)
______________________________________________________________________________
Reported to
______________________________________________________________________________
Dangerous defects  (if applicable; worked out automatically in the app)
______________________________________________________________________________
Result *  (choose one)
☐ Nil defects
☐ Minor defects reported, safe to drive
☐ Dangerous defect: do not drive
4. Sign-off
Driver name *
______________________________________________________________________________
Driver signature
	



Fleet manager or supervisor  (if applicable)
______________________________________________________________________________
Repair carried out and by whom  (if applicable)
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
Date repaired  (if applicable)
______________________________________________________________________________
	If applicable: The repair date is before the date of the check. Check both dates.



Supervisor signature  (if applicable)
	



Vehicle Inspection Checklist. Printable copy from the SiteSurvey form library. Fill it in on a phone, with photos and signatures: sitesurvey.app/forms/vehicle-inspection-checklist/




