Ventilation Ductwork Cleaning Record
A ventilation ductwork inspection and cleaning record (TR19 Air): system and hygiene grade, visual inspection, deposit tests before and after, sections cleaned, access panels, filters, fire dampers, photos and report.
1. System
Project
______________________________________________________________________________
Client
______________________________________________________________________________
Site *
______________________________________________________________________________
Site address
______________________________________________________________________________
Date *
______________________________________________________________________________
Time
______________________________________________________________________________
Technician *
______________________________________________________________________________
Company
______________________________________________________________________________
System (AHU or fan reference and area served) *
______________________________________________________________________________
System  (choose one)
☐ Supply     ☐ Extract     ☐ Recirculation
Cleanliness class (risk)  (choose one)
☐ High (for example laboratories, hospital treatment areas)
☐ Medium (for example offices, hotels, schools)
☐ Low (for example storage and technical rooms)
	BESA TR19 Air, released in April 2024, is the specification for the internal cleanliness of general ventilation systems. Inspection starts with a visual check of whether cleaning is needed, and deposit tests show whether surfaces are within acceptable limits. Regulation 5 of the Workplace Regulations 1992 requires mechanical ventilation systems in workplaces to be maintained, including cleaned as appropriate.



2. Inspection and clean
Visual inspection result  (choose one)
☐ Clean: no cleaning needed     ☐ Cleaning needed     ☐ Contaminated: specialist clean
Deposit test units  (choose one)
☐ Microns (deposit thickness test)     ☐ g/m² (weight of dust)
Deposit test before
______________________________________________________________________________
Deposit test after
______________________________________________________________________________
Sections cleaned  (copy this block for each one)
Section or run *
______________________________________________________________________________
Length (m)
______________________________________________________________________________
Method  (choose one)
☐ Rotary brush     ☐ Compressed air     ☐ Hand clean     ☐ Vacuum
Before photos  (photos: attach, or note the file names)
______________________________________________________________________________
After photos  (photos: attach, or note the file names)
______________________________________________________________________________
Total length cleaned (m)  (worked out automatically in the app)
______________________________________________________________________________
Access panels fitted or used
______________________________________________________________________________
Filters changed or cleaned?
☐ Yes     ☐ No
Fire dampers checked and reset?
☐ Yes     ☐ No
3. Report
Defects (damaged ductwork, insulation, missing access, mould)
______________________________________________________________________________
______________________________________________________________________________
______________________________________________________________________________
Next inspection due
______________________________________________________________________________
Site manager name
______________________________________________________________________________
Site manager signature
	



Completed by *
______________________________________________________________________________
Signature
	



Ventilation Ductwork Cleaning Record. Printable copy from the SiteSurvey form library. Fill it in on a phone, with photos and signatures: sitesurvey.app/forms/ductwork-cleaning-record/




